

EE462 & EE464 Project: Design of a SM-PMSM Variable Frequency Drive with Matlab/Simulink

Hakkı GÜLCÜ

Tel: +90 534 397 29 66

mail: [hakkigulcu35@gmail.com](mailto:hakkigulcu35@gmail.com)

2093862

Özgür

Tel: +90 535 938 69 20

mail: [xxxxxxx](mailto:bulbulbahar@gmail.com)

209xxxxx

**Supervisor:** Ozan KEYSAN & Emine BOSTANCI

Date of Submission: 02.06.2019

# Introduction

The aim of project is to design a SM-PMSM Variable Frequency Drive with respect to given parameters below by using matlab Simulink program.

𝑃𝑛𝑜𝑚𝑖𝑛𝑎𝑙 = 80 𝑘𝑊

T𝑛𝑜𝑚𝑖𝑛𝑎𝑙 = 300 𝑁𝑚

𝑛𝑚𝑎𝑥 = 7000 𝑟𝑝𝑚

Pole number: p=8

𝐹𝑙𝑢𝑥 𝑙𝑖𝑛𝑘𝑎𝑔𝑒: 𝜆𝑃𝑀 = 0.2 Vs (Wb-t)

𝐿𝑑 = 𝐿𝑞 = 500 uH

𝐼𝑛𝑜𝑚𝑖𝑛𝑎𝑙 = 250 𝐴 (peak)

Phase resistance 𝑅𝑠 = 50 mOhm

Equivalent inertia of the system: 𝐽𝑒𝑞 = 10 kg m2

Ignore windage and friction losses.

The available supply is a three-phase AC source (50 Hz, 400Vl-l) and the PM is a surface-mount motor. Assume a 3-phase full-bridge diode rectifier is connected to the grid.

# Part A: Pre-design Stage

## Calculation of the rated speed and torque of the PMSM.

Wbase=== 266.67 rad/sec , Nbase=2546.48

T= 𝜆𝑃𝑀\*iq Where nomimal base Torque condition,İq=İnominal =250 A , İd=0

Then T=1.5\*4(pp)\*0.2\*250 = 300Nm where it is also given in parameters.

## Calculation of the maximum applied electrical frequency and choose a switching frequency for your inverter

We=2\*π\*f , then frequency=

where from part a We(max)= is found 733 rad/sec,

fmax==116.67 Hz

Swich frequency ?